**Q40 Fencing & Gates Specification**

*To be read in conjunction with Preliminaries/General conditions*

Description: Multi threat security fence system

Standard: LPS 1175 A1, B3, C5 or D10 (SR1, SR2, SR3 or SR4) Issue 8

 IWA 14-1:2013 V/7200(N3C)/80/90:8.5

 Secured By Design

Manufacturer: CLD Systems info@cld-systems.com

Tel. 01270 764751 www.cld-systems.com

**Product Reference:** **CLD Rampart 50 Multi Threat Security Fence**

Panel type: Shallow foundation hostile vehicle mitigation system for use with CLD Securus S1, S2, S3 or S4 panels. See separate specification sheets for mesh fence panels

Wire diameter: HVM: Rope diameter 22mm galvanised or 22.15mm coated

Height: HVM: 1370mm from finished floor level

Finish: See separate specification sheet for fence panel information.

HVM: Can be coated with black high density polyethylene (HDPE) coating to 150 microns.

Installation: 400mm depth with 50mm concrete blinding. Tolerance +/- 10mm.

Concrete C40/50

specification:

Warranty: Minimum of 15 years against manufacturing defects.

Notes: All dimensions are nominal, for further information please contact CLD Fencing Systems.

Information is correct at time of production. As part of our policy of continuous improvement, we reserve the right to alter product specification without notice.